ABBREVIATIONS

The following abbreviations are used in this manual.

A/C | = | Air Conditioner
A/C | = | Air Conditioning
A/F | = | Air Fuel
A/T | = | Automatic Transaxle
A/T | = | Automatic Transmission
ABS | = | Anti-Lock Brake System
AC | = | Alternating Current
ACIS | = | Acoustic Control Induction System
ACM | = | Active Control Engine Mount
ACS | = | Automatic Clutch System
ADD | = | Automatic Disconnecting Differential
AFS | = | Adaptive Front-Lighting System
AHC | = | Active Height Control
AICV | = | Air Intake Control Valve
AIRV | = | Air Bypass Valve
AVC-LAN | = | Audio Visual Communication - Local Area Network
BA | = | Brake Assist
BACS | = | Boost Altitude Compensational Stopper
BEAN | = | Body Electronics Area Network
C/B | = | Circuit Breaker
C/P | = | Coupe Type
CAN | = | Controller Area Network
CD | = | Compact Disc
CDI | = | Capacitive Discharge Ignition
CIS | = | Commonwealth of Independent States
COMB. | = | Combination
CPU | = | Central Processing Unit
D/A | = | Digital/Analog
DC | = | Direct Current
DIFF. | = | Differential
DIS | = | Direct Ignition System
DLC3 | = | Data Link Connector 3
DRL | = | Daytime Running Light
DSP | = | Digital Signal Processor
DVD | = | Digital Versatile Disc
EB | = | Electrical Brake
EBD | = | Electronic Brake Force Distribution
EC | = | Electrochromic
ECT | = | Electronic Control Transmission
ECT | = | Electronically Controlled Transmission
ECT-i | = | Electronically Controlled Transmission-intelligent
ECU | = | Electronic Control Unit
EDU | = | Electronic Driving Unit
EFI | = | Electronic Fuel Injection
EGR | = | Exhaust Gas Recirculation
EHPS | = | Electro Hydraulic Power Steering
EI | = | Electronic Ignition
EMPS | = | Electric Motor Power Steering
EPS | = | Electric Motor Power Steering
ES | = | Easy & Smooth
ESA | = | Electronic Spark Advance
ETCS-i | = | Electronic Throttle Control System-intelligent
EV | = | Electric Vehicle
EVAP | = | Evaporative Emission
E-VRV | = | Electronic Vacuum Regulating Valve
FL | = | Fusible Link
FPU | = | Fuel Pressure Up
FWD | = | Front Wheel Drive
G.C.C. | = | Gulf Cooperation Council
GPS | = | Global Positioning System
GSM | = | Global System for Mobile Communications
GVWR | = | Gross Vehicle Weight Rating
H/B | = | Hatchback Type
H/T | = | Hardtop Type
HID | = | High Intensity Discharge
HV | = | Hybrid Vehicle
HWS | = | Heat Windshield
IAC | = | Idle Air Control
IACV | = | Intake Air Control Valve
IC | = | Integrated Circuit
IIA | = | Integrated Ignition Assembly
INT | = | Intermittent
IRS | = | Independent Rear Suspension
ISC | = | Idle Speed Control
ISCV | = | Idle Air Control Valve
J/B | = | Junction Block
L/B | = | Liftback Type
LCD | = | Liquid Crystal Display
LED | = | Light Emitting Diode
LH | = | Left-Hand
LHD | = | Left-Hand Drive
LSPV | = | Load Sensing Proportioning Valve
M/C | = | Magnetic Clutch
M/T | = | Manual Transaxle
M/T | = | Manual Transmission
MFI | = | Multiport Fuel Injection
MPX | = | Multiplex
O/D | = | Overdrive
ORVR | = | On-Board Refueling Vapor Recovery
PPS | = | Progressive Power Steering
PTC | = | Positive Temperature Coefficient
PTO | = | Power Take Off
PZEV | = | Partial Count Zero Emission Vehicle
R/B | = | Relay Block
RH | = | Right-Hand
RHD | = | Right-Hand Drive
RSES | = | Rear Seat Entertainment System
S/D | = | Sedan Type
SCB | = | Supercharger Bypass
SCV | = | Swirl Control Valve
SFI | = | Sequential Multiport Fuel Injection
SMR | = | System Main Relay
SNS | = | Satellite Navigation System
SOC | = | State of Charge
SPEC. | = | Specification
SRS | = | Supplemental Restraint System
SW | = | Switch
TC | = | Torque Control
TCS | = | Traction Control System
TDC | = | Top Dead Center
TDCL | = | Total Diagnostic Communication Link
TDCL | = | TOYOTA Diagnostic Communication Link
TEMP. | = | Temperature
TEMS | = | TOYOTA Electric Modulated Suspension
TFT | = | Toyota Free-Tronic
TP | = | Throttle Positioner
TRAC | = | Traction Control
TRC | = | Traction Control
TVIP | = | TOYOTA Vehicle Intrusion Protection
T-VIS | = | TOYOTA-Variable Induction System
TVSS | = | TOYOTA Vehicle Security System
TWC | = | Three Way Catalytic Converter
U.K. | = | United Kingdom
VGRS | = | Variable Gear Ratio Steering
VRV | = | Vacuum Regulating Valve
VSC | = | Vehicle Stability Control
VSV | = | Vacuum Switching Valve
VVL | = | Variable Valve Lift
VVT | = | Variable Valve Timing
VVT-i | = | Variable Valve Timing-intelligent
VVTL | = | Variable Valve Timing and Lift
VVTL-i | = | Variable Valve Timing and Lift-intelligent
w/ | = | With
W/G | = | Wagon Type
w/o | = | Without
2WD | = | Two Wheel Drive Vehicles
2WS | = | Two Wheel Steering System
4WD | = | Four Wheel Drive Vehicles
4WS | = | Four Wheel Steering System

*The titles given inside the components are the names of the terminals(terminal codes) and are not treated as being abbreviations.